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CT-42 Label Printer
Key Features
· 1-inch high-precision 300  dpi print head, delivering DPI sharper, clearer and more refined printing
· Rubber-coated housing design with 1.5 m drop resistance; sealed dust-proof cover ensures clean and stable printing
· Support PC editing software (Windows/macOS) and mobile apps (Android/iOS) for seamless cross-platform collaboration
· 2600 mAh lithium battery, providing long-lasting power and worry-free operation for outdoor and on-site use
· All-in-one consumable design for quick and easy installation; automatically matches label templates to improve operational efficiency

Technical Specification
	ITEM
	SPECIFICATION

	Printing Method
	thermal transfer

	Resolution
	300dpi

	Print Width
	1 inch (25.4 mm)

	Print Speed
	25.4mm/s

	Dimensions
	146*118*62mm

	Weight
	600g

	Battery
	2600mAh

	Continuous Printing Time
	2.5 hours (25 °C,12.5% print density)

	Charging Port
	Type-C

	Interface
	USB (type-C), Bluetooth

	Operation Method
	MobileAPP(MakelD Label Pro)/PC Label design

	Cutter
	Manual Cutter

	Consumables
	All-in-one consumables

	Accessories
	Magnet, belt clip(optional)

	Operating Environment
	0- 40 °C, 20 %- 9 0 % RH (non-condensing)

	Storage Environment
	-20°C- +6 0 °C, 5%- 9 3% RH(non-condensing)



Cable Labels
MateriaI: Matte PP film
Features: Tear-resistant, high-temperature resistant, and resistant to common chemical solvents
AppIication: Pigtail, Ethernet CabIe, Powe r CabIe, Feeder Cable and other cables
	Model
	Size(axb+c)
	Specifications
	Color

	WQS-02F(107)/G
	25mm*38mm+40mm
	100 pcs/case
	White/Red/Yellow/Blue/Green

	WQS-07F(107)/G
	25mm*38mm+25mm
	123 pcs/case
	White/Red/Yellow/Blue/Green
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GUANGGU INC.

Add.: 1F of block A, Tangyuege, Xi'an Software Park, Keji 2 Road, Yanta District, Xi'an, Shaanxi, Chinal 710075)

Tel.: O0O86-29-88115682
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