
SAT-18EXB Mini OTDR
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Applicable Scenarios
1. Access Network (FTTx/FTTH)
2. Metro Network (Short to Medium Span)
3. Data Center & Equipment Room
4. Field Deployments & Emergency Restoration
5. Industry Specific Networks (Power, Railway, Metro)
6. Pre-construction Survey & Preliminary Acceptance

Key Features
· Suitable for FTTx and other access network, test fiber’s length, loss, breakpoint etc. 
· 3.5“colorful LCD screen, utral-light design for easily carrying,
· 8 in 1: OTDR, OLS, OPM, VFL, iOTA(Event Map),RJ Sequence, RJ length and LED Lighter.
· Universal connector: FC/SC/ST/LC for choice.
· Large internal storage with 600 results, and extensible TF card, USB wire can upload the testing results to PC for printing.
· Built-in 4000mAh li-ion rechargeable battery, can charge by any USB charger, suitable for long-term field working.

General Specification
	Screen
	3.5“Colorful LCD screen

	Connect Port
	FC/UPC(SC、ST available)

	Com. Port
	Micro USB*1

	Results Storage
	Internal：≥600；External：TF Card; 
File type: SOR Standard file format

	Battery Life
	stand by>7.5h； testing >4h

	Power Supply
	3.7V, 4000mAh lithium battery; 
Power adapter:5VDC, 2A.

	Working Environments
	Working temperature: 0~+50℃，<95%RH

	Dimensions/Weight
	173mm*82mm*37mm,  <350g



Technical Specification
	Dynamic Range
	24/22dB

	Wavelength
	1310nm/1550nm±20nm

	Fiber Type
	SM (G.652)

	Event Dead Zone
	3m

	Attenuation Dead Zone
	8m

	Pulse Width
	3ns to10us

	Distance Range
	500m to 60km

	Measurement Accuracy
	± (1m+sample space+0.005%*measurement distance)

	Linearity
	±0.2 dB/dB

	Sample Points
	16k~128k

	Sample Resolutions
	0.05m~8m

	IOR
	±3dB

	VFL
	Output Power 
	10mW

	
	Wavelength
	650±20nm

	
	Working Mode
	CW/1Hz/2Hz

	
	Connect Port
	FC/SC/ST

	Power Meter
	Wavelength
	800nm to 1700 nm

	
	Calibrated wavelength
	850/980/1300/1310/1490/1550/1625 nm

	
	Measurement range
	-50 to +26 dBm

	Laser 
Source
	Working Wavelength
	1310nm/1550nm±20nm

	
	Output Power
	≥-5dBm

	
	Frequency
	270Hz /330Hz /1kHz /2kHz   

	RJ45
	Testing Distance
	300m




Packing List
	No.
	Description
	Qty
	Remarks

	1
	Main Unit
	1
	With battery

	2
	Power Adapter
	1
	

	3
	Data Cable
	1
	

	4
	CD 
(Including analysis software & user manual)
	1
	

	5
	Operation Manual
	1
	

	6
	SC/UPC Connector
	1
	

	7
	Test Report
	1
	

	8
	Certificate of Conformity / 
After-sales Warranty Card
	1
	

	9
	Cleaning Wipes
	10
	

	10
	Instrument Carry Case
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