SAT-1AS E1 BER Tester
Key Features

· 5 inch LCD with backlight, the largest screen in the industry
· Handheld, rugged design, easy to operation
· Particular history and real-time LED indicator design, find troubles more clearly
· Smart auto configuration feature
· Alarm and Histogram analysis for troubleshooting
· Multi-task operation at the same time
· Store 20 test results and 9 test configurations, with power-off memory
· Automatically power on/off testing by programmable timer
· Powerful PC software supports download results to PC, data analysis, report generation, printing, etc.
· Software updating

Key Functions

Normal testing
Pass through testing 
Audio frequency testing
Applications for E1
· Service-interrupted error testing
· On-line service error testing
· Framed and unframed signals generation and reception
· 2Mbit/s unframed error performance testing
· 2Mbit/s framed N×64Kbit/s channel error testing
· Bit error, coding error, frame error, CRC error and E-bit error testing
· Signal loss alarm, AIS alarm, framed remote alarm, multi-framed remote alarm, out-of-frame, and pattern loss alarm
· Frequency offset transmitting
· Voice channel signal level and frequency testing
· Pattern slip testing
· Pass through testing
· Audio frequency testing
· Voice monitoring
· Signal state display, Voice channel content display, Voice channel busy / idle indication
· Alarm and error histogram analysis
· Time slot content analysis, drop and insert signal on each time slot
· Framed content analysis
· G. 821/G. 826/M. 2100 performance analysis
· Multi errors and alarms inserting
· Three input modes (terminating, bridging and monitoring)
· [bookmark: _GoBack]Provides two clock options (internal and picking-up)
