[image: ]SAT-3C01 Pen Type Visual Fault Locator

· Fast locate the broken point in fiber
· 2.5mm universal connector
· Glint or CW output
	Model
	Out power

	SAT-3c04-10
	10mW

	SAT-3c04-20
	20mW

	SAT-3c04-30
	30mW
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