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[image: ]SAT-3E Optical Laser Source
Key Features 
· High sensitivity, multi output power
· Multi wavelengths optional, up to four wavelengths on two ports
· Automatic power-off, off time setting range 30~90mins
· Low battery alarm
· LCD display
· New-type conductive rubber switch, suitable for different operation environments.



Technical Specifications
	[bookmark: OLE_LINK1][bookmark: OLE_LINK2]Model
	3E
3E04
3E05
3E06
3E07
3E08

	Working
Wavelength(nm)
	1310/1550nm

	Output Power (dBm)
	850/1300/1310/1550/1490/1625: -6 (error:±0.2)

	Output Tone
	850/1300/1310/1550 /1490/1625: CW, 270Hz, 1KHz, 2KHz; 650: CW

	Spectrum Width
	 5nm

	Output Stability
	±0.03dB/15min; 0.05dB/8H

	Optical Identity Distance
	5km; 10km/15km optional (650nm)

	Display
	LCD

	Optical Interface
	FC, SC, ST

	Power Supply
	AA alkaline batteries

	Operating Temperature
	-10---+50°C

	Size
	L*H*W:140*72*38mm, 0.3kg
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