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SAT-3F series handheld optical laser source is mainly used for fiber optic link continuity test, visual fault locator and loss test. The output power can be adjusted by 6dB and has multiple optional wavelengths. It is widely used in fiber optic construction and maintenance, fiber optic communication, fiber optic sensing, optical CATV and other fields. It can also be used for insertion loss and splitting ratio test of passive devices such as optical splitters, circulators, optical couplers and optical switches.
Features
· Support single wavelength, and accept combined wavelength customization.
· Support output of CW and multiple modulation
· Output power is adjustable range from 6dB by 1dB step
· RJ45 sequence test
· RJ45 tracker test(optional)
· Auto shut-down time can be set.
Specification
	Models
	3F01
	[bookmark: OLE_LINK26]3F02
	3F03

	Wavelength
	[bookmark: OLE_LINK25]1310/1550±20nm
	1310/1490/1550±20nm
	850/1300±20nm

	Output power
	-5dBm

	Power adjustable range 
	0~6dB

	Power adjustable step
	1 dB

	Stability
	[bookmark: OLE_LINK30]≤±0.2dB/15min (pre-heat after 15 min.)

	Working mode
	CW/270Hz/330Hz/1kHz/2kHz/ID/TWINS

	Connector
	FC/SC

	RJ45 sequence range
	≤300m

	RJ45 tracker 
	Test range  ≤300m, Mode  digital search; support live link search

	General Parameters

	Screen
	Segment code screen

	Power
	Rechargeable li-ion 1500mAh battery

	Auto power -off 
	10 min./30 min./60 min./120 min.

	Continuous working
	≥24h

	Weight
	235g

	Size
	140mmX32mmx73mm

	Environment
	Working:-10C+50℃; Storage: -40C+70℃, 
Humidity: 0~95% non-condensing 
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