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SAT-4F series optical power meter is integrated function with power meter, RJ45 sequence, flashlight, laser source, RJ45 tracker etc., it’s mainly used for continuous optical signal power test, optical link loss test and continuity test. 
It is widely applied in optical cable construction and maintenance, optical fiber communication, optical cable sensing, optical CATV and other fields.
Features
· 10 wavelength power testing;
· PASS/FAIL threshold can be set.
· Wavelength ID and frequency recognition,
· RJ45 sequence test.
· Optional for RJ45 tracker and VFL.
· Auto shutdown time can be set
· Data upload and analysis
Specification
	Model
	4F01
	4F02

	Wavelength
	800nm-1700nm
	800nm~1700nm

	Connector
	FC/SC
	FC/SC

	Detector type
	InGaAs
	InGaAS

	Power range
	-70~+10dBm
	-50dBm-+30dBm

	Accuracy
	±5%

	Calibrated wavelength
	850/980/1270/1300/1310/1490/1550/1577/1625/1650nm

	Resolution
	0.01dB

	Identified frequency
	270Hz、330Hz、1kHz、2kHz

	Storage
	1000

	Custom wave
	50 

	Wavelength recognition
	support

	VFL (Optional)
	Wavelength 650±30nm; Output power ≥10mw;
Mode: CW/1Hz/2Hz; Connector: universal FC/SC/ST.

	RJ 45 sequency
	Range ≤300m

	RJ45 tracker (optional)
	Range ≤300m; mode: digital tracking; live to line  Support

	General Parameter

	Screen
	Segment code screen

	Power
	Rechargeable li-ion 1500mAh battery

	Auto power -off 
	10 min./30 min./60 min./120 min.

	Continuous working
	≥24h

	Weight
	235g

	Size
	140mmX32mmx73mm

	Environment
	Working:-10C+50℃; Storage: -40C+70℃, 
Humidity: 0~95% non-condensing
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