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[bookmark: OLE_LINK35][bookmark: OLE_LINK9]SAT-4FWM CWDM Optical Power Meter
[image: ]CWDM optical power meter is a full-featured palm-sized CWDM optical network channel detector, which is mainly used to measure and monitor the power of up to 6 or 18 CWDM channels. The test power value can be displayed in bar graph or list mode. It is specially designed and developed for the installation, acceptance and maintenance of CWDM optical networks, and has become a necessary special tool for the maintenance and installation of CWDM access networks.

Features
· Support 6 or 18 channels wavelength power test
· 3.5 inch TFT LCD, resolution 320*480.
· Single channel power information can be viewed.
· Easy to carry and easy to operate.
· Display test data in column graph or list mode.
· OPM/VFL/RJ45 sequence/cable length/cable search
· Can be charged y power bank
· User define PASS/FAIL threshold


Specification
	Model
	4FWM-6
	4FWM-18

	CWDM Optical power Mater

	Detector type
	InGaAS

	Connector
	FC/UPC

	Wave range
	1270~1370nm/1271~1371nm
	[bookmark: OLE_LINK38]1270~1610nm/1271~1611nm

	Power 
	-70~+10dBm

	Channel qty.
	6
	18

	Channel spacing
	20nm

	Channel band pass
	±6.5nm

	Power resolution
	0.01dB

	Power accuracy
	±0.5dB

	Series test loss(dB)
	≤1.5

	Return loss
	>45dB

	Isolation of adjacent channel
	≥25dB

	Unit
	mW/μW/nW/dBm/dB (REF)

	Optical Power Meter
	Calibration wavelength: 850/980/1300/1310/1490/1550/1625/1650nm
Power Range: -70~+10dBm, -50~+26dBm(optional)
Connector: FC/PC

	Visual Fault Locator
	Working wavelength :650nm±20nm; universal FC/SC/ST
Output power: ≥10mW; Mode: CW/1Hz/2Hz; Connector: 2.5mm 

	RJ45
	RJ45 length:≤300m;  RJ45 sequence:≤300m;RJ45 search≤300m



	General parameters

	Display
	3.5 inch 320*480 color LCD 

	Storage
	≤1000 

	Data interface
	Micro USB

	Power supply
	Polymer 3.7V,4000mAh;       Adapter:5VDC,2A

	Battery life
	Standby>20 hours；testing>12 hours

	Weight
	350g

	Size
	173mm×82mm×37mm

	Environment
	Working:-10C+50℃; Storage: -40C+70℃, 
Humidity: 0~95% non-condensing
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