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SAT-6C can detect optical signal presence/type and direction anywhere on fibers during optical network deployment, maintenance and troubleshooting. With non-destructive macro-bend detection technology, it introduces no damage to tested fiber or interference to the service on fiber. SAT-6C is able to identify wide-spectrum signals (such as signals in CATV system) and can be used in SONET/SDH & DWDM systems tests.

Key Applications:
1. Confirming live fibers – Clamp onto a fiber before maintenance. "Light + service signal" means do not cut or unplug; "no light" means safe to proceed. Prevents accidental service disruption.
2. Checking transmission direction – Verifies Tx/Rx orientation during patch cord management, service migration, or route verification in ODFs, avoiding reversed connections.
3. Identifying signal types – Detects modulation frequencies (270 Hz, 1 kHz, 2 kHz) to locate target fibers in dense cabling, especially with a modulated light source.
4. [image: ]Wide deployment – Used in carrier equipment rooms, base stations, and data centers; distinguishes downstream/upstream signals in PON networks; serves as a safety tool for live cable operations in military, power, and railway private networks.


Key Features
· Fiber types: 250μm, 900μm,
 2mm/3mm jacketed fiber
· Universal for SM&MM
· Support flashlight and VFL
· Indication of signal presence, strength and direction
· CW/MOD tones detection
· Buzzer indication
· Handheld & sturdy





Specification
	Model
	SAT-6C

	ldentified Wavelength Range
	800~1700nm

	Detector Type
	Φ1mm InGaAs 2 pcs

	Signal Type
	CW, 270Hz±5%, 1kHz±5%, 2kHz±5%

	Display
	Signal presence, Signal strength, Signal direction, MOD frequency

	Adapter Type
	250um (for bare fiber), 900um/ 2mm/3mm jacketed fiber

	Signal Direction
	Left & Right LED

	Signal Direction Test Range
	-40+13dBm

	Signal Frequency
	270Hz,1kHz,2kHz

	Power Supply
	6F22ND/6LR61

	Operating Temperature
	-10 ~ 60℃

	Storage Temperature
	-25 ~70℃

	Relative Humidity
	0 ~ 95% (Non-condensing)

	Weight
	255g

	Dimensions (H×W×T)
	195×80×30mm

	VFL 
	Output power:1mw; Testing range:3~5km; Wavelength:650nm;
Laser type: LD;

	Flashlight
	Support
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