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PON power meter is part of most essential tool for all technicians installing or maintaining PON networks. PON power meters are well designed for all kinds of demanding applications on fiber measurement with different functions and parameters. With a rugged design, SAT-7E series PON power meters are built for top ruggedness and versatility, perfect for the harshest test conditions to verify the continuity and evaluated fiber link transmission quality.

[bookmark: _GoBack]Key Features
1. Automated PASS/FAIL assessment.
2. Quick and efficient visual inspection.
3. Providing distinct power values for 1310nm,1490nm,1550nm.
4.Pass through measurement.
5. Simultaneously measure and display the concurrent voice, data and video signals on different PON architectures.
6. Manual calibration.
7. One-year warranty and three-year recommended calibration interval.

Specifications

	Measurement Range(dBm)
	1310nm: -40---+10dBm;  1490nm:-50--+10dBm; 1550nm:-50--+25dBm

	Pass Through Loss
	< 1.5dB

	Accuracy
	±0.2 dB(burst signal:±0.5dB)

	Threshold Sets
	10

	Data Storage
	100

	Connector
	SC/PC(or customize)

	Auto Power Off
	No operation in 10 minutes(can be cancelled), low  battery energy

	Battery Charger
	Yes

	Connect to PC
	Optional function

	Manual Calibration
	Yes

	Operating Time
	Above 36 hours

	Power Supply
	3xAA batteries or AC/DC power supply adapter

	Size
	L x H x W: 190 x 90 x 40mm,

	Weight
	About 450kgs

	Storage Temperature
	-20℃——+60℃, <90%RH

	Operating Temperature
	-10℃——+50℃, <90%RH



