SAT-7F  PON Power Meter
SAT-7F PON power meter integrates FTTx/PON power meter, VFL, RJ45 sequence, cable length, and RJ45 tracker. 
Features
· 3.5 inch TFT screen
· 1310/1490/1550nm in PON system can be tested.
· Support function VFL/ RJ45 sequence/cable length/ RJ45 tracker.
· Auto shutoff time can be set
· PASS/FAIL threshold can be set
Specification
	Wavelength
	1310±50 nm
	1490±15 nm
	1550±10 nm

	Isolation 1310nm
	--
	>40dB
	>40dB

	Isolation 1490nm
	>40 dB
	--
	>40dB

	Isolation 1550nm
	>40 dB
	>40dB
	--

	Dynamic range
	-35~+10 dBm
	-40~+12 dBm
	-40~+25dBm

	Uncertainty
	≤0.5dB

	Insertion Loss
	≤1.5dB

	Display resolution
	0.01dB

	Connector
	FC/UPC (SC can be used)

	VFL (Optional)
	Wavelength 650士30nm; Output power ≥10mw;
Mode: CW/1Hz/2Hz; Connector: Universal FC/SC/ST.

	RJ 45 sequency
	Range ≤300m 

	RJ45 length
	≤300m

	RJ45 tracker
	Range ≤300m; mode:digital tracking; live to line  Support
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	Display
	3.5inch color LCD 

	Storage
	≤1000 

	Data interface
	Micro USB

	Power supply
	Polymer 3.7V,4000mAh
Adapter:5VDC,2A

	Battery life
	Standby>20 hours；testing>12 hours

	Weight
	350g

	Size
	173mm×82mm×37mm

	Environment
	Working:-10C+50℃; Storage: -40C+70℃, 
Humidity: 0~95% non-condensing



