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SAT-AC Battery Conductance Tester(配夹子线的图片)
Key Functions
· Test the battery voltage and conductance online.

· Battery conductance and voltage out of range alarm.

· All the battery parameters are marked by group No. to make the user manage the data expediently.
· PC software analysis the battery to carry out tracking historical analysis of battery system.

Technical Specification
	Model
	SAT-AC

	Conductance Test Range
	100S-19990S

	Voltage Test Range
	0.000~20.000V conductance & voltage                  20.000~25.000Vvoltage only or warring

	Measurement Precision
	Conductance: ±0.5%, rdg:±6dgt
Voltage: ±0.2%, rdg: ±6dgt

	Power Supply
	10.8V,2000mAh, rechargeable lithium battery

	Watt Consumption
	Work for 8 hours continuously

	Storage Capacity
	2G Micro SD 

	Display
	320 x 240 matrix dot LCD

	Size
	210 x 140 x 60 mm

	Weight
	1.2Kg

	Working Temperature
	-5℃~ +60℃

	Humidity
	90%RH


SAT-AR Battery Internal Resistance Tester(配探针线图片)

Function
1. Test the battery voltage and internal resistance online.

2. Battery internal resistance and voltage out of gauge alarm.

3. All the battery test results are marked by group no., user can manage the data conveniently.

4. PC software analysis the battery according to the history data.

Technical Specifications
	Model
	SAT-AR

	Testing range
	0.000~20.000V internal resistance & voltage
20.000~25.000Vvoltage only

	Testing voltage precision
	±0.2%rdg  ±6dgt

	Testing internal resistance range
	0.000mΩ-99.999mΩ

	Testing internal resistance precision
	±0.5%rdg  ±6dgt

	Communication mode
	SD card

	Display
	320 x 240 LCD

	Power supply
	10.8V,2000mAh, rechargeable lithium battery

	Size
	280 x 105 x 83 mm

	N．W
	1.2kg



