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Key Features: 
1. 7 inch large touch screen
2.10~600V wide-range design, can meet requirement for different voltage degree’s battery discharge testing, voltage can continuously adjust. 
3. Constant current discharge function, current can continuously adjust.
[bookmark: _Hlk69389095]4. Individual cell wireless monitor function, each module can monitor 12 single cells.
5. Support wireless battery cell monitor module and compatible with 2V/6V/12V 
individual cell type.
6. Comprehensive analysis software, can remotely control discharging.

Application Scenarios
1. Daily maintenance and management of batteries
2. Inspection, acceptance, and installation of newly received batteries
3. To provide a basis for scrapping batteries
4. Quality control of battery manufacturers


Optional Function:
Internal resistance testing function
Online Compensation discharge function

Specification

	Battery Group Voltage 
	24V/48V/72V/96V/110V/22V/240V/380V/480V

	Individual Cell Voltage
	2V/6V/12V

	Operating Mode
	Independently using, parallelly using, and remotely operating and morning.

	Discharge Voltage
	DC 10V~600V

	Discharge Current Range
	10~19V
	19~180V
	180~300V
	300~600V

	
	80A
	120A
	80A
	50A

	Battery Group Current Accuracy
	1%

	Battery Group Voltage Accuracy
	0.5%

	Individual Cell Voltage Accuracy
	0.2%

	Individual Cell Range
	0.5V~16V (Resolution 1mv)

	Discharge Time
	0~99H59Min.

	Working Voltage
	AC: 220V

	Cooling Mode
	Forced air cooling

	Package 
	Aluminum alloy trolley case& outer wooden case

	Temperature
	Operating temperature: -5~50℃;
 storage temperature: -40~70℃

	Dimension
	Accord to specific model




