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SAT-CD Series Battery Charge Tester
Key Feature
1. Intelligent 3 degree charging, auto switch for equalized/floating charging, constant current/voltage.
2. Portable design, small volume, light weight ,easy to move.
3. Upload the test data to PC to generate test report, easily check the battery performance. 
4. USB port, 2G large data storage space.

Application Scenarios

1. Daily maintenance and management of batteries
2. Inspection, acceptance, and installation of newly received batteries
3. To provide a basis for scrapping batteries
4. Quality control of battery manufacturers

Technical specification 
	Model
	SAT-CD 48/10
	SAT-CD 48/20
	SAT-CD 110/04
	SAT-CD 220/04
	SAT-CD 380/01

	Battery Group Voltage Range
	40-60V
	95-150V
	190V-300V
	350V-450V

	Charging Current
	100A
	200A
	40A
	40A
	10A

	Control precision
	Charge current ≤ ±1%; group terminal voltage ≤ ±0.1%; cell voltage ≤ ±0.1%

	PC communication
	RS485 interface, USB interface

	Data storage capacity
	Built-in SD card with a capacity of 8G and the USB flash drive with a capacity of 16G

	Work Environment

	Heat dissipation
	Forced air cooling

	Temperature
	Working rage: -5-50℃  Storage temperature: -40-70℃

	Humidity
	Relative humidity 0-90% (40±2℃)

	Working Power Supply

	Voltage
	Power supply: single-phase AC220V (-20%-+30%), 
frequency: 45-65Hz; charging power supply: refer to nameplate parameters or case label

	Electric strength test
	Input-housing: 2200Vdc 1min; Input-output: 2200Vdc 1min; Output-housing: 700Vdc 1min


Remark: Accept customization service. The charge current range from 40A to 300A. Please contact with for more details. 

