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SAT-DC500 Series Battery Charge and Discharge
Key Feature
1. 5 in 1: Charge, discharge, cell monitor, online monitor, and battery activator.
2. Individual cell wireless monitor function, each module can monitor 12 single cells.

3. USB port, 2G large data storage space.

4. Dual-CPU collaborative working, guarantee the security and accuracy during testing.

5. Can suspend or edit parameters during discharging, instead of stopping testing.
Application Scenarios

1. Daily maintenance and management of batteries
2. Inspection, acceptance, and installation of newly received batteries
3. To provide a basis for scrapping batteries
4. Quality control of battery manufacturers

Technical Specification  
	Available Battery Group 
	48V
	110V
	220V
	380V

	Charging voltage
	40-60V
	95-150v
	190-300V
	350-450V

	Charging current
	10-150A
	1-80A
	1-40A
	1-20A

	Discharging voltage 
	10-60V
	85-135V
	80-270V
	300-460V

	Discharging current
	0-150A
	0-200A
	0-100A
	0-60A

	Current Resolution
	1%

	Voltage Resolution
	0.5%

	Individual Cell Voltage Resolution
	0.2%

	Individual Cell Voltage
	0.5V~16V(Resolution:1mV)

	Charge and Discharging Time
	0~99H59Min

	Power Supply
	AC:220V

	Cooling Mode
	Forced air cooling

	Package 
	Aluminum alloy trolley case& outer wooden case

	Temperature
	Operating temperature: -5~50℃;

 storage temperature: -40~70℃

	Dimension
	Accord to specific model


Note: Please consult us if you need tester for other voltage levels and current levels. 

Customization is available as per customer’s voltage and current requirement

