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SAT-G5 series optical power meter is integrated function with power meter, laser source, RJ45 sequence, flashlight, laser source, RJ45 tracker etc., it’s mainly used for continuous optical signal power test, optical link loss test and continuity test. 
It is widely applied in optical cable construction and maintenance, optical fiber communication, optical cable sensing, optical CATV and other fields. 
Features
· 10 wavelength power testing;
· Set with reference power and display relative power
· Wavelength ID and frequency recognition
· Support output of CW and multiple modulation
· Output power is adjustable range from 6dB by 1dB step
· RJ45 sequence test, RJ45 tracker test(optional)
· PASS/FAIL threshold can be set.
· Auto shut-down time can be set.
· Data upload and analysis.
Specification
	Optical Power Meter
	Wavelength :800nm-1700nm
Calibrated wavelength:850/980/1270/1300/1310/1490/1550/1577/1625/1650nm
Frequency: 270Hz、330Hz、1kHz、2kHz
Connector: FC/SC;   Detector type: InGaAs
Power range: -70~+10dBm/50dBm~+30dBm;         Accuracy: ±5%

	Laser Source
	Wavelength :1310/1550±20nm;   1310/1490/1550±20nm
Output power: -5dBm; Power range: 0~6dB; Connector: FC/SC
[bookmark: OLE_LINK29]Working mode: CW/270Hz/330Hz/1kHz/2kHz/ID/TWINS

	VFL (Optional)
	Wavelength 650士30nm; Output power ≥10mw;
Mode: CW/1Hz/2Hz; Connector: Universal FC/SC/ST.

	RJ 45 sequency
	Range ≤300m

	RJ45 tracker
(optional)
	Range:≤300m; mode: digital tracking;  live to line :Support

	General Parameters

	Screen
	Segment code screen

	Power
	Rechargeable li-ion 1500mAh battery,

	Auto power -off 
	10 min./30 min./60 min./120 min.

	Weight
	235g

	Size
	140mmX32mmx73mm

	Environment
	Working:-10C+50℃; Storage: -40C+70℃, 
Humidity: 0~95% non-condensing
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