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SAT-IA Intelligent Battery Activator
Function
· Activation function
· Check discharge function
· Charge function
· Real-time data memory
· Data upload and export
· Automatic protection function

Application Scenarios
1. Daily maintenance and management of batteries
2. Inspection, acceptance, and installation of newly received batteries
3. To provide a basis for scrapping batteries
4. Quality control of battery manufacturers

Specification
	Measurement Type of Cell Voltage
	2V/6V/12V;

	Measurement Range of Cell Voltage
	2V:0～3V; 6V: 4-8V; 12V:4-15V 

	Resolution of Cell Voltage
	2V: 0.001V; 6V: 0.01V; 12V:0.01V

	Voltage Testing Accuracy
	0.5%

	Working Range of Charge and Discharge Current
	2A~100A

	Control Accuracy of Charge and Discharge Current
	0.1A

	Current Testing Accuracy
	1%

	Battery Capacity Check Range
	2V:20-1000Ah;6V:20-200Ah:12V:20-300Ah;

	Working Voltage
	AC 220±15%

	Communication Mode
	RS232 communication and USB communication

	Cooling Mode
	Refrigeration by blasting

	Working Environment
	Temperature: 0℃～40℃    
Humidity: 20%～80%RH

	Storage Condition
	-20℃～70℃  package and storage

	Display Mode
	LCD with High-brightness 

	External Dimensions(W×H×L)
	450mm×190mm×585mm

	Weight
	11kg

	Carry Method
	Portable type, move with roller wheel
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