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Key features
· 2-in-1 multifunction cleaver can operation fiber cutting 
and thermal stripping by only one machine
· CNC machining with all mental machine body, 
fine workmanship
· Small size, user-friendly
· Built-in 2200mAh battery, type-C charging port
· 3 gears of temperature settings
· Use ribbon fiber holder can realize cleave 12 cores and strip 12 cores simultaneously, improve working efficiency
Specification
	Cladding Diameter
	125μm

	Applicable Fiber Type
	Fanout fiber /bare fiber/ribbon fiber/ invisible fiber

	Cutting Length
	10~20+mm (Visual); 5~20+mm (Estimable)

	Average cutting Angle
	≤0.6°

	Fiber Holder
	4-in-1multifunction

	Battery Capacity
	7.4V /2200mAh

	Temperature Gears
	145℃/160℃/70℃

	Countdown time
	5 secs

	Auto Power Off
	10 mins

	Power Supply
	5V 1A ，Type-C charging Port

	Blade edge width
	14mm

	Dimension
	57W*83D*66H(mm)

	Weight 
	450g

	Standard Configuration
	Fiber Cleaver*1; Protection carry case *1;
User Manual (QR code) *1; Brush *1; Allen Wrench*2;
USB Charging cable*1; Warranty Card*1

	Optional Accessories
	Fiber Off-cut Collector; Ribbon Fiber Holder
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