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Magnification 400X
Resolution(um) surpass 1.0
Optical Fiber Visual range(um) 0.316%0.285
inspector Dimension(um) 235(W)*95(D)*30(H)
Image Sensor 1/3 480
Storage Temperatrue ~18'C~35C
Weight(kg) 0.11
i Image size(mm) 22
Pixels 307200
Frequency 25FPS
LCD screen 960*240 LCD
Video Video output mode NTSC/PAL
Playback Format AVI
35-inch LCD Compatible memory cards TF
display Capacity 8GB
User interface
usB 1.1/2.0
Hard disk format FAT32
AC adapter DC 5V/2A
Power supply Internal Battery Lithium battery 4000Mah
Media Player >7
Weight(kg)/W*D*H(mm) 0.085/78%22*56
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Support APC

Support UPC's FC,
Support APC's SC male&female
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