[bookmark: OLE_LINK3][bookmark: OLE_LINK5][bookmark: OLE_LINK9][bookmark: OLE_LINK10][bookmark: OLE_LINK1][bookmark: OLE_LINK2]1).LED Light
2). Wide measurement range, High resolution
3).SM or MM applications
4). 2.5mm universal connector
5).850/1300/1310/1490/1550/1625nm
6). Auto power off (can be cancelled)

Specification

	[bookmark: OLE_LINK7][bookmark: OLE_LINK8]Model
	SAT-4EXT
	SAT-4EXC

	Display Range
	1310/1490/1550/1625:-70--+10 dBm
850/1300： -60--+6 dBm
	1310/1490/1550/1625:-50--+26 dBm
850/1300： -40--+26 dBm

	Accuracy
	± 0.2dB

	Calibrated Wavelengths
	850nm/1300nm/1310nm/1490nm/1550/nm/1625nm

	Display Resolving Power 
	0.01dB
	

	Linearity
	± 0.2 dB

	OPM Connector
		2.5mm universal 

	VFL Connector
	2.5mm universal 

	VFL Output(Optional)
	1mW or 10mW, CW and Glint

	LED Light
	SOS code output

	Automatic Power Off
	No operation in 10 minutes (can be cancelled),
 Low battery energy.	

	Battery Charge
	Yes

	Battery Life
	Above 60 hours(OPM)

	Size
	105mm X 52mm X24mm

	Weight
	About 100g

	Storage Temperature
	-20---+60 ℃

	Operating Temperature
	-10---+50 ℃

	Humidity
	<90%RH

	Elevation
	0---5000m



4EXT=OPM(-70---+10 dBm)+VFL(1nw)/No VFL
4EXC=OPM(-50---+26 dBm)+VFL(1nw)/No VFL



[bookmark: OLE_LINK4][bookmark: OLE_LINK6]Aitelong released a new model of optical power meter to meet the market requirement , for which is named 
SAT-4EX Mini optical power meter. It's featured with:
· LED Light
· Wide measurement range,high resolution 
· SM or MM application
· 2.5mm universal connector
· 850/1300/1310/1490/1550/1625nm
· Auto power off(can be cancelled)
· One-year warranty
Aitelong has released a new product SAT-4EX Mini optical power meter,which is in smaller size, easier operation, and more beautiful 
shell.
