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SAT-AG Series Battery Discharge Tester
Key Features
1. Constant-current discharge function, current can be adjusted;
2. Input terminal overvoltage protection, prompts on the LCD; 
3. Buzzer alarm for battery voltage reverse polarity protection;
4. Overcurrent protection, prompts on the LCD; 
5. Single battery voltage acquisition function, each model for 12 cells.
6. 2Gbit internal data storage space, USB port for testing data download.
7. Comprehensive analysis software for PC.
8. 7inch color touch TFT screen with high performance.

Application Scenarios

1. Daily maintenance and management of batteries
2. Inspection, acceptance, and installation of newly received batteries
3. To provide a basis for scrapping batteries
4. Quality control of battery manufacturers

Optional Function:

1. Internal resistance testing function

2. Online Compensation discharge function

Technical Specifications

	Model No.
	AG 24/05
	AG 24/15
	AG 48/15
	AG 48/30
	AG 110/05
	AG 220/10
	AG 380/03
	AG 480/10

	Output Voltage
	24V
	24V
	48V
	48V
	110V
	220V
	380V
	480V

	Output Current
	50A
	150A
	150A
	300A
	50A
	100A
	30A
	100A

	Control Accuracy
	Discharge current: ≤±1%; battery pack’s terminal voltage: ≤ ±0.1%;
 single battery voltage: ≤±0.05%

	Communication With The Host PC
	RS485 interface

	Data Storage Capacity
	2Gbit FLASH

	Cooling
	Forced air cooling

	Working Environment
	Operating temperature: -5~50℃; storage temperature: -40~70℃
Relative humidity: 0~90% (40±2℃)

	Voltage
	Single-phase three-wire system: 220V AC (–20%~+30%); frequency: 45~65Hz;

	Withstand Voltage Test
	Input--casing: 2200Vdc 1min; Input--output: 2200Vdc 1min;

Output--casing: 700Vdc 1min

	AC Output
	Male socket in line with the applicable national standard, applicable to 1~1.5mm2 cable

	DC Output
	25mm2 cable quick plug (red: positive; black: negative)


*The external load can raise capacity check.                           *Accept customization service.

